**Drivers shall check the status of the items listed below as part of the Vehicle Daily Inspection. Alert the VMU of any and all discrepancies.**

**Basic equipment:**

* Hydrogen Peroxide Fire extinguisher (usually under Driver seat)
* First aid kit
* Flashlight and spare batteries
* Spare tire(s), Jack, handle, lug wrench, key for tire locks
* Warning triangles; flares (when available)
* Battery jumper cables
* Foot or electric pump (plugs into cigarette lighter)
* HF radio mike (if radio equipped – conduct radio check)

**Situational equipment:**

* Fuel jerry can(s) (for long trips where fuel may not be readily available / overland evacuation)
* Potable water or water filtering system (for long trips / overland evacuation)
* Equipment to extricate from mud/sand/snow (as necessary, e.g. shovels, 10-20m X 5mm cable or tow strap)
* Winch control (if winch is installed)
* Come-along and cable
* Blankets and food

**Documents:**

* All vehicle documents (copies or originals as per local laws: title, registration, taxes, insurance, registration)
* Maps (indicate: mined roads, checkpoints, evacuation routes, etc.)
* Vehicle logbook (including multiple Vehicle Log Sheets and Vehicle Daily Inspection Checklists)
* Radio frequencies and call signs list (if radio equipped)
* Emergency contact list (e.g., CRS staff, hospital, consulate, police, etc.).
* Itinerary and any copies of written approval for travel (as required)
* Discharge of Responsibility form (for non-CRS passengers)
* CRS’ mission statement in local language